Quick Installation Guide

The below steps assume that you have installed the screen reader and windows in their default locations. 

Open the "manual_english v5.0".
Install Seika braille display driver (refer to Chapter3 of manual_english v5.0).
Install the Seika patch program and configure your screen reader (refer to Chapter 5 for Jaws, Chapter 6 for Windoweyes, Chapter 7 for HAL, Chapter 8 for Virgo, Chapter 9 for NVDA).
