Quick Installation Guide

The below steps assume that you have installed the screen reader and windows in their default locations. 

Open the "manual_english v3.4".
Install Seika braille display driver (refer to Chapter3 of manual_english v3.4).
Install the Seika patch program and configure your screen reader (refer to Chapter 4 for Jaws, Chapter 5 for Windoweyes, Chapter 6 for HAL, Chapter 7 for Virgo, Chapter 8 for NVDA).
